CONTINUOUS BEAM

CONTINUOUS BARS NOT LESS THAN 1 AREA OF

4

BARS AT COL FACE

A=L1/3

A=L1/3

A=L1/3

Ld

2d

2d

2d

STIRRUP SPACING=d/4 OR

100mm OR 8dia WHICH EVER IS THE LEAST

ALL DIMENSIONS ARE IN CM

|  |  |  |
| --- | --- | --- |
| Karthika Viswambharan | CONTINUOUS BEAM | |
| S6CB | DRW NO : 4 | SCALE : |
| REG NO: NSS21CE067 | MARK : |  |
| DATE : | SIGNATUR E |  |